**Project # 070112 - High Pressure Mud Pump Fluid Ends**

Technical questionnaire:

* + Does your product have a safety mechanism to prevent fluid end components from being removed from the fluid modules while the pump is under pressure?
  + Does your product offer quick change wear plates, or does the liner retention system body need to be removed to access the wear plate?
  + Does your product offer hammerless valve, liner, strainer, and pony rod systems?
  + Please state what the liner loads for 5.5”/5.25”/5” liners at maximum pump pressure will be.
  + Does your company have experience with engaging certifying authorities on such projects? If so, please provide a list of certifying authorities utilized.
  + Does your company have the means to complete the Hibernia fluid end replacement project, as noted above, in 6-months?